aula23-profe
    description: Computer
    width: 64 bits
    capabilities: smp vsyscall32
  *-core
       description: Motherboard
       physical id: 0
     *-memory
          description: System memory
          physical id: 0
          size: 3328MiB
     *-cpu
          product: AMD A6-6400K APU with Radeon(tm) HD Graphics
          vendor: Advanced Micro Devices [AMD]
          physical id: 1
          bus info: cpu@0
          size: 3225MHz
          capacity: 3900MHz
          width: 64 bits
          capabilities: fpu fpu_exception wp vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp x86-64 constant_tsc rep_good nopl nonstop_tsc cpuid extd_apicid aperfmperf pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 popcnt aes xsave avx f16c lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs xop skinit wdt lwp fma4 tce tbm topoext perfctr_core perfctr_nb cpb hw_pstate ssbd vmmcall bmi1 arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold cpufreq
     *-pci:0
          description: Host bridge
          product: Family 15h (Models 10h-1fh) Processor Root Complex
          vendor: Advanced Micro Devices, Inc. [AMD]
          physical id: 100
          bus info: pci@0000:00:00.0
          version: 00
          width: 32 bits
          clock: 66MHz
        *-generic UNCLAIMED
             description: IOMMU
             product: Family 15h (Models 10h-1fh) I/O Memory Management Unit
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 0.2
             bus info: pci@0000:00:00.2
             version: 00
             width: 32 bits
             clock: 33MHz
             capabilities: cap_list
             configuration: latency=0
        *-display
             description: VGA compatible controller
             product: Richland [Radeon HD 8470D]
             vendor: Advanced Micro Devices, Inc. [AMD/ATI]
             physical id: 1
             bus info: pci@0000:00:01.0
             version: 00
             width: 32 bits
             clock: 33MHz
             capabilities: vga_controller bus_master cap_list rom
             configuration: driver=radeon latency=0
             resources: irq:27 memory:c0000000-cfffffff ioport:f000(size=256) memory:feb00000-feb3ffff memory:c0000-dffff
        *-multimedia:0
             description: Audio device
             product: Trinity HDMI Audio Controller
             vendor: Advanced Micro Devices, Inc. [AMD/ATI]
             physical id: 1.1
             bus info: pci@0000:00:01.1
             version: 00
             width: 32 bits
             clock: 33MHz
             capabilities: bus_master cap_list
             configuration: driver=snd_hda_intel latency=0
             resources: irq:28 memory:feb44000-feb47fff
        *-pci:0
             description: PCI bridge
             product: Family 15h (Models 10h-1fh) Processor Root Port
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 4
             bus info: pci@0000:00:04.0
             version: 00
             width: 32 bits
             clock: 33MHz
             capabilities: pci normal_decode bus_master cap_list
             configuration: driver=pcieport
             resources: irq:25 ioport:e000(size=4096) memory:fea00000-feafffff ioport:d0000000(size=1048576)
           *-network
                description: Ethernet interface
                product: RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
                vendor: Realtek Semiconductor Co., Ltd.
                physical id: 0
                bus info: pci@0000:01:00.0
                logical name: eth0
                version: 06
                serial: 74:d4:35:79:94:41
                size: 1Gbit/s
                capacity: 1Gbit/s
                width: 64 bits
                clock: 33MHz
                capabilities: bus_master cap_list ethernet physical tp mii 10bt 10bt-fd 100bt 100bt-fd 1000bt 1000bt-fd autonegotiation
                configuration: autonegotiation=on broadcast=yes driver=r8169 duplex=full firmware=rtl8168e-3_0.0.4 03/27/12 ip=172.31.23.197 latency=0 link=yes multicast=yes port=MII speed=1Gbit/s
                resources: irq:16 ioport:e000(size=256) memory:fea00000-fea00fff memory:d0000000-d0003fff
        *-sata
             description: SATA controller
             product: FCH SATA Controller [IDE mode]
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 11
             bus info: pci@0000:00:11.0
             logical name: scsi4
             version: 40
             width: 32 bits
             clock: 66MHz
             capabilities: sata ahci_1.0 bus_master cap_list emulated
             configuration: driver=ahci latency=32
             resources: irq:19 ioport:f190(size=8) ioport:f180(size=4) ioport:f170(size=8) ioport:f160(size=4) ioport:f150(size=16) memory:feb4f000-feb4f7ff
           *-cdrom
                description: DVD-RAM writer
                product: CDDVDW SH-224DB
                vendor: TSSTcorp
                physical id: 0.0.0
                bus info: scsi@4:0.0.0
                logical name: /dev/cdrom
                logical name: /dev/cdrw
                logical name: /dev/dvd
                logical name: /dev/dvdrw
                logical name: /dev/sr0
                version: SB01
                capabilities: removable audio cd-r cd-rw dvd dvd-r dvd-ram
                configuration: ansiversion=5 status=nodisc
        *-usb:0
             description: USB controller
             product: FCH USB OHCI Controller
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 12
             bus info: pci@0000:00:12.0
             version: 11
             width: 32 bits
             clock: 66MHz
             capabilities: ohci bus_master
             configuration: driver=ohci-pci latency=32
             resources: irq:18 memory:feb4e000-feb4efff
        *-usb:1
             description: USB controller
             product: FCH USB EHCI Controller
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 12.2
             bus info: pci@0000:00:12.2
             version: 11
             width: 32 bits
             clock: 66MHz
             capabilities: ehci bus_master cap_list
             configuration: driver=ehci-pci latency=32
             resources: irq:17 memory:feb4d000-feb4d0ff
        *-usb:2
             description: USB controller
             product: FCH USB OHCI Controller
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 13
             bus info: pci@0000:00:13.0
             version: 11
             width: 32 bits
             clock: 66MHz
             capabilities: ohci bus_master
             configuration: driver=ohci-pci latency=32
             resources: irq:18 memory:feb4c000-feb4cfff
        *-usb:3
             description: USB controller
             product: FCH USB EHCI Controller
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 13.2
             bus info: pci@0000:00:13.2
             version: 11
             width: 32 bits
             clock: 66MHz
             capabilities: ehci bus_master cap_list
             configuration: driver=ehci-pci latency=32
             resources: irq:17 memory:feb4b000-feb4b0ff
        *-serial
             description: SMBus
             product: FCH SMBus Controller
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 14
             bus info: pci@0000:00:14.0
             version: 14
             width: 32 bits
             clock: 66MHz
             configuration: driver=piix4_smbus latency=0
             resources: irq:0
        *-ide
             description: IDE interface
             product: FCH IDE Controller
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 14.1
             bus info: pci@0000:00:14.1
             version: 00
             width: 32 bits
             clock: 66MHz
             capabilities: ide isa_compat_mode pci_native_mode bus_master
             configuration: driver=pata_atiixp latency=32
             resources: irq:17 ioport:1f0(size=8) ioport:3f6 ioport:170(size=8) ioport:376 ioport:f100(size=16)
        *-multimedia:1
             description: Audio device
             product: FCH Azalia Controller
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 14.2
             bus info: pci@0000:00:14.2
             version: 01
             width: 64 bits
             clock: 33MHz
             capabilities: bus_master cap_list
             configuration: driver=snd_hda_intel latency=32
             resources: irq:16 memory:feb40000-feb43fff
        *-isa
             description: ISA bridge
             product: FCH LPC Bridge
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 14.3
             bus info: pci@0000:00:14.3
             version: 11
             width: 32 bits
             clock: 66MHz
             capabilities: isa bus_master
             configuration: latency=0
        *-pci:1
             description: PCI bridge
             product: FCH PCI Bridge
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 14.4
             bus info: pci@0000:00:14.4
             version: 40
             width: 32 bits
             clock: 66MHz
             capabilities: pci subtractive_decode bus_master vga_palette
        *-usb:4
             description: USB controller
             product: FCH USB OHCI Controller
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 14.5
             bus info: pci@0000:00:14.5
             version: 11
             width: 32 bits
             clock: 66MHz
             capabilities: ohci bus_master
             configuration: driver=ohci-pci latency=32
             resources: irq:18 memory:feb4a000-feb4afff
        *-usb:5
             description: USB controller
             product: FCH USB OHCI Controller
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 16
             bus info: pci@0000:00:16.0
             version: 11
             width: 32 bits
             clock: 66MHz
             capabilities: ohci bus_master
             configuration: driver=ohci-pci latency=32
             resources: irq:18 memory:feb49000-feb49fff
        *-usb:6
             description: USB controller
             product: FCH USB EHCI Controller
             vendor: Advanced Micro Devices, Inc. [AMD]
             physical id: 16.2
             bus info: pci@0000:00:16.2
             version: 11
             width: 32 bits
             clock: 66MHz
             capabilities: ehci bus_master cap_list
             configuration: driver=ehci-pci latency=32
             resources: irq:17 memory:feb48000-feb480ff
     *-pci:1
          description: Host bridge
          product: Family 15h (Models 10h-1fh) Processor Function 0
          vendor: Advanced Micro Devices, Inc. [AMD]
          physical id: 101
          bus info: pci@0000:00:18.0
          version: 00
          width: 32 bits
          clock: 33MHz
     *-pci:2
          description: Host bridge
          product: Family 15h (Models 10h-1fh) Processor Function 1
          vendor: Advanced Micro Devices, Inc. [AMD]
          physical id: 102
          bus info: pci@0000:00:18.1
          version: 00
          width: 32 bits
          clock: 33MHz
     *-pci:3
          description: Host bridge
          product: Family 15h (Models 10h-1fh) Processor Function 2
          vendor: Advanced Micro Devices, Inc. [AMD]
          physical id: 103
          bus info: pci@0000:00:18.2
          version: 00
          width: 32 bits
          clock: 33MHz
     *-pci:4
          description: Host bridge
          product: Family 15h (Models 10h-1fh) Processor Function 3
          vendor: Advanced Micro Devices, Inc. [AMD]
          physical id: 104
          bus info: pci@0000:00:18.3
          version: 00
          width: 32 bits
          clock: 33MHz
          configuration: driver=k10temp
          resources: irq:0
     *-pci:5
          description: Host bridge
          product: Family 15h (Models 10h-1fh) Processor Function 4
          vendor: Advanced Micro Devices, Inc. [AMD]
          physical id: 105
          bus info: pci@0000:00:18.4
          version: 00
          width: 32 bits
          clock: 33MHz
     *-pci:6
          description: Host bridge
          product: Family 15h (Models 10h-1fh) Processor Function 5
          vendor: Advanced Micro Devices, Inc. [AMD]
          physical id: 106
          bus info: pci@0000:00:18.5
          version: 00
          width: 32 bits
          clock: 33MHz
     *-pnp00:00
          product: PnP device PNP0c01
          physical id: 2
          capabilities: pnp
          configuration: driver=system
     *-pnp00:01
          product: PnP device PNP0c02
          physical id: 3
          capabilities: pnp
          configuration: driver=system
     *-pnp00:02
          product: PnP device PNP0c02
          physical id: 4
          capabilities: pnp
          configuration: driver=system
     *-pnp00:03
          product: PnP device PNP0c02
          physical id: 5
          capabilities: pnp
          configuration: driver=system
     *-pnp00:04
          product: PnP device PNP0501
          physical id: 6
          capabilities: pnp
          configuration: driver=serial
     *-pnp00:05
          product: PnP device PNP0c02
          physical id: 7
          capabilities: pnp
          configuration: driver=system
     *-pnp00:06
          product: PnP device PNP0b00
          physical id: 8
          capabilities: pnp
          configuration: driver=rtc_cmos
     *-pnp00:07
          product: PnP device PNP0c02
          physical id: 9
          capabilities: pnp
          configuration: driver=system
     *-pnp00:08
          product: PnP device PNP0c02
          physical id: a
          capabilities: pnp
          configuration: driver=system
